{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Foglio2","Foglio3","Dati"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Foglio2","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":true,"merged":[]}

{"sheet":"Foglio3","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":true,"merged":[]}

{"sheet":"Dati","index":2,"n_rows":17,"n_cols":16,"rows_kept":17,"cut":false,"hidden":false,"merged":[]}
["Ø Tubo (mm)","Lunghezza tubi (metri)","Q.tà pannelli","Q.tà bollitori","Selezione modello","Litri totale pannello","Selezione Accumulo","Litri serpentina accumulo","Volume  ","Testo","N° taniche","Modello pannelli","Litri pannello","Modello Bollitori","Superfice serpentina m2","Litri Liquido solare"]
["22","21","2","2","SB+20 V",{"$f":"(VLOOKUP(E2,L1:M8,2,FALSE)*C2)","v":3.8},"UBVT 200 SC",{"$f":"(VLOOKUP(G2,N1:P17,3,FALSE)*D2)","v":16.2},{"$f":"CEILING((((A2/2)/1000)*((A2/2)/1000)*3.14*B2*1000)+F2+H2,2)","v":28},{"$f":"CONCATENATE(CEILING((((A2/2)/1000)*((A2/2)/1000)*3.14*B2*1000)+F2+H2,2),\" litri di liquido solare BAXI già diluito\")","v":"28 litri di liquido solare BAXI già diluito"},{"$f":"CONCATENATE(\"Per riempire correttamente l'impianto è necessario utilizzare \",CEILING(I2/10,1),\" taniche da 10 litri di liquido SOLARE premiscelato BAXI\")","v":"Per riempire correttamente l'impianto è necessario utilizzare 3 taniche da 10 litri di liquido SOLARE premiscelato BAXI"},"SB+20 V",1.9,"UBVT 200 SC",1.2,8.1]
[null,null,null,null,null,null,null,null,null,null,null,"SB+20 O",2.2999999999999998,"UBVT 200 DC",1.2,8.1]
[null,null,null,null,null,null,null,null,null,null,null,"SB+25 V",2.2999999999999998,"UBVT 300 SC",1.5,10.1]
[null,null,null,null,null,null,null,null,null,null,null,"SB+25 O",2.7,"UBVT 300 DC",1.5,10.1]
[null,null,null,null,null,null,null,null,null,null,null,"SOL200 V",1.2,"UBVT 400 SC",1.8,12.1]
[null,null,null,null,null,null,null,null,null,null,null,"SOL250 V",1.4,"UBVT 400 DC",1.8,12.1]
[null,null,null,null,null,null,null,null,null,null,null,"SOL250 O",1.8,"UBVT 500 DC",2.5,16.899999999999999]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"UBSI 300",1.5,10.1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"UBSI 500",2.5,16.899999999999999]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"UB 800 DC",2.7,18.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"UB 1000 DC",3,20.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"UB 1500 DC",3.4,22.9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"UB 2000 SC",4.5999999999999996,31]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"UB 2000 DC",4.5999999999999996,31]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"UB TT 300",1.2,8.1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"UB TT 600",2.5,16.899999999999999]